[Contents] [Prev] [Next] [Index] [Report an Error]

# show ldp vpls

#### Syntax

show [ mpls ] ldp vpls [ vplsName | neighbor ipAddress ] [ filter ]

#### Release Information

Command introduced in JUNOSe Release 8.2.0.

#### Description

Displays MPLS configuration information for a VPLS instance that uses LDP as the signaling protocol. You can display information for a specific VPLS instance, for a specific neighbor address, or for all VPLS instances configured on the router.

#### Options

- mpls—Specifies optional keyword for compatibility with non–E Series implementations
- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command
- ipAddress—IP address of a neighbor in the VPLS domain
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Monitoring LDP-Related Settings for VPLS in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]