[Contents] [Prev] [Next] [Index] [Report an Error]

# ip igmp querier-timeout

#### Syntax

ip igmp querier-timeout seconds

no ip igmp querier-timeout

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the time that the interface waits before declaring itself as the querier. The no version restores the default value, twice the query interval.

#### Options

- seconds—Time interval between the last query from the previous router and the first query from this interface

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]