[Contents] [Prev] [Next] [Index] [Report an Error]

# ip igmp static-group

#### Syntax

[ no ] ip igmp static-group groupAddress

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Assigns an interface to handle all multicast traffic for a group. The interface sets no timers for this group. The no version removes the group from the interface.

#### Options

- groupAddress—Address of the group

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]