[Contents] [Prev] [Next] [Index] [Report an Error]

# ppp initiate-ip

#### Syntax

[ no ] ppp initiate-ip

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Initiates IPv4 for passive clients. By default, PPP creates IP instances when it receives client requests. The no version disables initiation.

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]