[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Failure Messages for Secure Policies

#### Purpose

Display failure messages and information for secure policies. This command and the output are visible only to authorized users—the mirror-enable command must be enabled before using this command. All normal E Series system log messages are suppressed for packet mirroring-related policy operations.

#### Action

To display information for secure policies:

    host1#show mirror log

       Time       Mirror-ID      Session-ID   User          Error Status
    ----------- ---------------- ---------- ---------- ----------------------
    TUE FEB 03  8976             1923       suresh@aol no secure polic
    2004 18:35                              .com       ies available
    :43 UTC

    TUE FEB 03  8976             1924       219040@aol out of memory
    2004 18:35                              .com
    :39 UTC
    TUE FEB 03  8976             1924       not applic analyzer 1.1.1.1 is unr
    :30 UTC                                 able       eachble in virtual rou
                                                       ter default

#### Meaning

Table 62 lists the show mirror log command output fields.

Table 62: show mirror log Output Fields

Field Name | Field Description
--- | ---
Time | Day, date, and time of failure
Mirror-ID | Unique identifier of the mirrored session
Session-ID | Unique identifier of the user session
User | User login name
Error Status | Description of error condition

#### Related Topics

- show mirror log

[Contents] [Prev] [Next] [Index] [Report an Error]