> - Downloads
> - show l2tp dial-out

> # show l2tp dial-out

> #### Syntax

> show l2tp dial-out [ [ detail ] [ state operState ] | summary ] [ filter ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Displays the chassis-wide configuration, operational state, and statistics for L2TP dial-out.

> #### Options

> - detail—Displays configuration, states, and statistics
> - operState—One of the following operational states:
>   - inService
>   - initIncomplete
>   - restricted
> - summary—Displays aggregate counts for virtual routers, targets, and sessions in each of the possible operational and administrative states
> - filter—See Filtering show Commands

> #### Mode

> Privileged Exec

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.