> - Downloads
> - show ip interface
> - Related Topics
> - Monitoring the QoS Configuration of IP Interfaces
> - Monitoring the Policy Configuration of IP Interfaces
> - Monitoring the Packet Mirroring Configuration of IP Interfaces

> # show ip interface

> #### Syntax

> show ip interface [ vrf vrfName ]
> { { [ brief | detail | other | show-virtual-router [ virtualRouterName ] ]
> [ interfaceType interfaceSpecifier ] } | summary } [ delta ] [ filter ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> show-virtual-router keyword and virtualRouterName variable added in JUNOSe Release 7.3.0.
> other keyword added in JUNOSe Release 8.0.0.

> #### Description

> Displays current state of all IP interfaces or the IP interfaces you specify. The default is all interface types and all interfaces.

> #### Options

> - vrfName—Name of the VRF
> - brief—Displays a brief summary of IP status and configuration information
> - detail—Shows a detailed display of IP status and configuration information
> - other—Shows hidden interfaces and routes to the local address that are used internally so that from a given CE you can now ping the local address of any VRF that has a VPN overlapping a VPN to which the CE belongs
> - virtualRouterName—Name of the virtual router
> - interfaceType—Interface type; see Interface Types and Specifiers
> - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
> - summary—Shows a detailed summary of IP status and configuration
> - delta—Displays baselined statistics
> - filter—See Filtering show Commands

> #### Mode

> Privileged Exec, User Exec

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.