[Contents] [Prev] [Next] [Index] [Report an Error]

# Setting Timeouts for Assigned IP Subscriber Sessions

To set timeouts for assigned IP subscriber sessions in the SAE configuration:

1. From configuration mode, access the SAE configuration statement that configures subscriber sessions.
   `
   [edit]
   user@host# edit shared sae configuration subscriber-sessions
   `
2. Specify the interval after which assigned IP subscriber sessions are deactivated if no service session is active.
   `
   [edit shared sae configuration subscriber-sessions]
   user@host# set assigned-ip-idle-timeout assigned-ip-idle-timeout
   `

#### Related Topics

- Overview of Session Management for VoIP Services
- Tracking and Controlling Subscriber and Service Sessions with SAE APIs
- Configuring Access to Subscriber Data
- Activating VoIP Services for Assigned IP Subscribers

[Contents] [Prev] [Next] [Index] [Report an Error]