[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Statistics for Specific JUNOSe Device Drivers (SRC CLI)

#### Purpose

Display statistics for a specific JUNOSe device driver.

#### Action

Use the following operational mode command:

`

show sae statistics device <name name> < (brief) >

`

For example:

`user@host> show sae statistics device name default@dryad`

    SNMP Statistics
    Add notification handle time       6
    Change notification handle time    0
    Client ID                          default@dryad
    Delete notification handle time    0
    Failover IP                        0.0.0.0
    Failover port                      0
    Handle message time                60
    Job queue age                      0
    Job queue time                     4
    Number message send                158
    Number of added jobs               9
    Number of add notifications        4
    Number of change notifications     0
    Number of delele notifications     0
    Number of managed interfaces       4
    Number of message errors           0
    Number of message timeouts         0
    Number of removed jobs             9
    Number of user session established 0
    Number of user session removed     0
    Router type                        JUNOSE COPS
    Up time                            172286
    Using failover server              false

#### Related Topics

- Troubleshooting Problems with Managing JUNOSe Routers
- Viewing Statistics for All JUNOSe Device Drivers (SRC CLI)
- Monitoring Interactions Between the SAE and the JUNOSe Router
- Viewing the State of JUNOSe Device Drivers (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]