[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the State Synchronization Plug-In Interface (C-Web Interface)

Some external plug-ins, such as the Admission Control Plug-In (ACP) application and the SAE plug-in agent for the NIC, support state synchronization with the SAE. The state synchronization plug-in interface allows external plug-ins to maintain the state of active subscriber, service, and interface sessions without having to store intermediate versions of the state locally.

To configure the state synchronization plug-in interface:

1. To configure the state synchronization plug-in interface:
   1. Click Configure, expand Shared>SAE, and then expand the SAE group for which you want to configure a plug-in.
   2. In the side pane, expand Configuration>Plug Ins, and then click State Synchronization.

      The State Synchronization pane appears.

   3. Enter information as described in the Help text in the main pane, and click Apply.
2. To configure the number of threads:
   1. Click Configure, expand Shared>SAE, and then expand the SAE group for which you want to configure a plug-in.
   2. In the side pane, expand Configuration>Plug Ins, and then click Manager.
   3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- For information about creating a plug-in instance for a group, see Creating Plug-In Instances (C-Web Interface).

[Contents] [Prev] [Next] [Index] [Report an Error]