[Contents] [Prev] [Next] [Index] [Report an Error]

# Specifying Router Initialization Scripts on the SAE with the CLI

Use the following configuration statements to specify router initialization scripts for JUNOSe routers:

`

shared sae configuration driver scripts {
  extension-path extension-path ;
  general general ;
  junose-pr junose-pr ;
  junose-xdr junose-xdr ;
}

`

To configure router initialization scripts for JUNOSe routers:

1. From configuration mode, access the configuration statements that configure router initialization scripts. In this sample procedure, the scripts are configured in the west-region group.
   `
   user@host# edit shared sae group west-region configuration driver scripts
   `
2. Specify the script for JUNOSe routers when the JUNOSe driver uses COPS-PR mode when connecting to the SAE.
   `
   [edit shared sae group west-region configuration driver scripts]
   user@host# set junose-pr junose-pr
   `
3. Specify the script for JUNOSe routers when the JUNOSe driver uses COPS-XDR mode when connecting to the SAE.
   `
   [edit shared sae group west-region configuration driver scripts]
   user@host# set junose-xdr junose-xdr
   `

   In COPS-XDR mode, the router does not send the network access server (NAS) IP address to the SAE. If your configuration requires this value, add the following line to a JUNOSe script:

   `
   import ERXnasip
   `
4. Configure a router initialization script that can be used for all types of routers that the SRC module supports.
   `
   [edit shared sae group west-region configuration driver scripts]
   user@host# set general general
   `
5. Configure a path to router initialization scripts that are not in the default location, /opt/UMC/sae/lib.
   `
   [edit shared sae group west-region configuration driver scripts]
   user@host# set extension-path extension-path
   `
6. (Optional) Verify your router initialization script configuration.

       [edit shared sae group west-region configuration driver scripts]
       user@host# show
       junose-xdr poolPublisher;

#### Related Topics

- Accessing the Router CLI
- Configuring the SAE to Manage JUNOSe Routers with the CLI
- Monitoring Interactions Between the SAE and the JUNOSe Router
- Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices

[Contents] [Prev] [Next] [Index] [Report an Error]