> - Downloads
> - Configuration Statements for Customized SRC SNMP Monitors
> - Related Topics
> - Configuring an SNMP Alarm on a C Series Controller (SRC CLI)
> - Example: SNMP Monitoring of Multiple MIB Objects
> - Configuring an SNMPv3 Security Name for SNMP Monitoring (SRC CLI)
> - SNMP Monitoring on C Series Controllers
> - For detailed information about each configuration statement, see the SRC PE CLI Command Reference

> ## Configuration Statements for Customized SRC SNMP Monitors

> Use the following configuration statements to configure the SNMP custom monitoring at the [edit] hierarchy level.

> `
> snmp monitor {
>   security-name security-name;
> }
>   snmp monitor alarm name{
>     interval interval;
>     sample-type (absolute-value | delta-value);
>     ignore-startup-alarm;
>     event event;
>     variable variable;
>     strict-oid;
>   }
>   snmp monitor alarm name boolean-test {
>     comparison (equal | unequal | less | less-or- equal | greater | greater-or-equal);
>     value value;
>   }
>   snmp monitor alarm name existence-test {
>     type (present | absent | changed);
>   }
>   snmp monitor alarm name threshold-test {
>     rising-threshold rising-threshold;
>     falling-threshold falling-threshold;
>   }
>   snmp monitor alarm name delta-discontinuity-check {
>     variable variable;
>   }
>   snmp monitor event namenotification {
>     oid oid;
>     strict-object [strict-object...];
>     wildcarded-object [wildcarded-object...];
>   }
>   snmp monitor event name snmp-set {
>     variable variable;
>     value value;
>     strict-oid;
>   }
> `

> #### Published: 2009-09-10

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.