[Contents] [Prev] [Next] [Index] [Report an Error]

# Adding JUNOSe Routers and Virtual Routers (C-Web Interface)

The SAE uses router and virtual router objects to manage interfaces on JUNOSe virtual routers. Each JUNOSe router in the SRC network and its virtual routers (VRs) must have a configuration.

There are several ways to add routers:

1. Detecting Operative JUNOSe Routers and Virtual Routers and Adding Them to the Network
2. Adding JUNOSe Routers Individually
3. Adding Virtual Routers Individually

## Detecting Operative JUNOSe Routers and Virtual Routers and Adding Them to the Network

If you add a router using the discover network feature, the software adds the IP address of the first SNMP agent on the router to respond to the discover request.

To add routers and JUNOSe VRs that are currently operative and have an operating SNMP agent:

1. Click Manage>Request>Network>Discovery.
2. Enter information as described in the Help text in the main pane, and click Apply.

## Adding JUNOSe Routers Individually

To add a router:

1. Click Configure, expand Shared, and then click Network.

   The Shared Network pane appears.

2. From the Create new list, select Device.
3. Type a name for the new device in the dialog box, and click OK.

   The Device pane appears.

4. From the Device Type list, select JUNOSe.
5. Enter information as described in the Help text in the main pane, and click Apply.

## Adding Virtual Routers Individually

To add a virtual router to an existing router:

1. Click Configure, expand Shared>Network, and then click a JUNOSe router.

   The Device pane appears.

2. From the Create new list, select Virtual Router.
3. Type a name for the new device in the dialog box, and click OK.

   The Virtual Router pane appears.

4. Click Create, enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring the SAE to Manage JUNOSe Routers (C-Web Interface)
- Adding JUNOSe Routers and Virtual Routers with the CLI
- For information about service scopes, see Configuring Service Scopes (SRC CLI)
- For information about local IP address pools, see Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices
- COPS Connection Between JUNOSe Routers and the SAE

[Contents] [Prev] [Next] [Index] [Report an Error]