[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Reject Actions (C-Web Interface)

You can configure reject actions for JUNOS filter policy rules. The reject action causes the router to discard a packet and send an ICMP destination unreachable message.

To configure a reject action:

1. In the side pane, select a JUNOS filter policy rule.
2. From the Create new list, select Reject. Type a name for the action, and click OK.
3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring Reject Actions (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]