[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring TCP Conditions (C-Web Interface)

To configure TCP conditions:

1. In the side pane, expand a traffic condition, and select TCP Condition.
2. Click Create, enter information as described in the Help text in the main pane, and click Apply.

To configure source and destination ports for TCP conditions:

1. In the side pane, expand TCP Condition>Source Port, and select Port.
2. Click Create, enter information as described in the Help text in the main pane, and click Apply.
3. In the side pane, expand TCP Condition>Destination Port, and select Port.
4. Click Create, enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring TCP Conditions (SRC CLI)
- Configuring Protocol Conditions (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]