[Contents] [Prev] [Next] [Index] [Report an Error]

# Changing NIC Configurations (C-Web Interface)

If you change the type of NIC resolution that you use in your network (for example, from the OnePop configuration scenario to the OnePopAllRealms configuration scenario), delete any existing data and specify a static DN that identifies the DN for the new NIC configuration scenario; otherwise, the new NIC configuration may not perform resolutions correctly.

To change the type of NIC resolution that you use in your network:

1. Disable the NIC:
   1. Click Manage>Disable.
   2. In the Component list in the main pane, select NIC, and click OK.
2. Delete the NIC configuration data for the existing configuration scenario from the directory.
   1. Click Manage>Request>NIC>Clear>Scenario Data.

      The Scenario Data pane appears.

   2. In the Slot box, enter the number of the slot that contains the NIC scenario configuration (typically, slot 0), and click OK.
3. Restart the NIC host:
   1. Click Manage>Restart.
   2. In the Component list in the main pane, select NIC, and click OK.
4. Configure the new NIC scenario.

#### Related Topics

- Configuring a NIC Scenario (C-Web Interface)
- Changing NIC Configurations (SRC CLI)
- Testing a NIC Resolution (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]