[Contents] [Prev] [Next] [Index] [Report an Error]

# Integrating IDP into an SRC Environment

How you integrate IDP into your SRC environment depends on whether or not you direct all traffic to an IDP sensor. If you direct all traffic to an IDP sensor by placing an IDP sensor in the network paths through which all incoming and outgoing subscriber traffic passes, you do not need to configure services and subscriptions to director traffic to a sensor, and do not need to monitor subsets of traffic. In this case, you can skip Steps 1 and 2 in the following procedure.

To integrate IDP into an SRC environment:

1. Configure services to direct traffic to IDP.

   See Configuring Services and Subscriptions to Integrate IDP.

2. Configure Surveillance Director to monitor groups of subscriber traffic.

   See Monitoring Subsets of Subscriber Traffic.

3. Configure actions to be taken for traffic that IDP identifies as malicious.

   See Defining Actions to Be Taken for Subscriber Traffic.

4. (Optional) Create an application, such as one to send e-mail notification to a subscriber about problem traffic that have sent or received.

   We provide a sample application to send an e-mail notification to a subscriber about the problem. See Sending E-Mail to Subscribers.

5. Create an SRC script for IDP Manager to complete the IDP integration with the SRC software.

   See Enabling SRC Actions from IDP Manager .

[Contents] [Prev] [Next] [Index] [Report an Error]