[Contents] [Prev] [Next] [Index] [Report an Error]

# Specifying Maximum Number of RADIUS Peers (SRC CLI)

The dynamic RADIUS server can maintain a certain number of peers.

To specify the maximum number of peers with the SRC CLI:

1. From configuration mode, access the SAE configuration statement that configures dynamic RADIUS options.
   `
   [edit]
   user@host# edit shared sae configuration dynamic-radius-server
   `
2. Specify the maximum number of peers maintained by the dynamic RADIUS server.
   `
   [edit shared sae configuration dynamic-radius-server]
   user@host# set maximum-cached-peer maximum-cached-peer
   `

#### Related Topics

- Configuring Packet-Mirroring Support in an SRC Network
- Defining RADIUS Attributes for Dynamic Authorization Requests with the SAE Core API
- Example: Using the Sample Packet-Mirroring Application
- Overview of Packet-Mirroring Services

[Contents] [Prev] [Next] [Index] [Report an Error]