> - Downloads
> - Configuring Source Grouped Networks (SRC CLI)
> - Related Topics
> - Before You Configure Classify-Traffic Conditions
> - Configuring Classify-Traffic Conditions
> - Configuring Source Networks (SRC CLI)
> - Configuring Source Grouped Networks (C-Web Interface)

> # Configuring Source Grouped Networks (SRC CLI)

> You can configure source networks in grouped format. For JUNOS ASP and JUNOSe IPv6 policy rules, you must enter source networks in grouped format.

> Use the following configuration statement to add source networks in a grouped format to a classify-traffic condition:

> `
> policies group name list name rule name traffic-condition name source-network group-network {
>   network-specifier network-specifier ;
> }
> `

> To add a grouped source network to a classify-traffic condition:

> 1. From configuration mode, enter the source network within a classify-traffic condition. For example:
>    `
>    user@host# edit policies folder junose group dhcp list in rule forward-dhcp traffic-condition client-dhcp source-network group-network
>    `
> 2. (Optional) Configure the IP address of the source network or host.

>    For JUNOS ASP policy rules, you must enter networks in the format <ip address>/<prefix length>. The <ip address>/<mask> format is rejected by the router.

>    For JUNOSe IPv6 policy rules, you must enter networks in the format <ipv6 address>/<prefix length>.

>    `
>    [edit policies folder junose group dhcp list in rule forward-dhcp traffic-condition client-dhcp source-network group-network]
>    user@host# set network-specifier network-specifier
>    `
> 3. (Optional) Verify your source network configuration.

>        [edit policies folder junose group dhcp list in rule forward-dhcp traffic-condition client-dhcp source-network group-network]
>        user@host# show
>        network-specifier gateway_ipAddress;

> #### Published: 2009-09-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.