[Contents] [Prev] [Next] [Index] [Report an Error]

## Example: Creating Router Interface Subscriber Session

Aggregate services or script services can be activated on a router instead of an interface or DHCP address. On JUNOSe routers that use the COPS-PR or COPS XDR router driver, the SAE automatically creates a router interface; and then a subscriber session as specified by the subscriber classification script.

For example, the following script searches for a router profile in the directory under ou=routers, retailerName=default, o=Users, o=umc, with a routerName attribute that matches the virtual router name (such as default@erx-node1).

    [edit shared sae group west-region subscriber-classifier rule rule-1]
    user@host#  show
    target ou=routers,retailername=default,o=Users,o=UMC??sub?(routerName=<-virtualRouterName->);
      condition {
        "interfaceName==\"Router\"";
      }

#### Related Topics

- Overview of Classification Scripts
- Overview of Configuring Classification Scripts
- Sending DHCP Options to the JUNOSe Router
- Assigning DHCP Addresses to Subscribers

[Contents] [Prev] [Next] [Index] [Report an Error]