[Contents] [Prev] [Next] [Index] [Report an Error]

# Modifying Congestion Points

By default, SRC ACP does not register changes in congestion points until you stop and restart SRC ACP. To modify the congestion point associated with a service without stopping and starting SRC ACP:

1. Make sure that no subscribers have subscriptions to services that use the congestion point you want to modify.
2. From configuration mode, access the configuration statement that configures SRC ACP connections to the services’ directory.
   `
   user@host# edit shared acp configuration ldap service-data
   `
3. Specify whether SRC ACP detects changes in the backbone congestion point for a service while SRC ACP is operative.
   `
   [edit shared acp configuration ldap service-data]
   user@host# set reload-congestion-points
   `
4. Wait for 30 seconds before you proceed to the next step.

   Depending on the value of the polling interval for directory eventing, SRC ACP may take up to 30 seconds to register the change to the reload-congestion-points option. If you modify the congestion point before SRC ACP registers the new setting for the reload-congestion-points option, SRC ACP will not register the change for the congestion point.

5. Modify the congestion point in the service definition.

   SRC ACP immediately registers the change.

6. From configuration mode, access the configuration statement that configures SRC ACP connections to the services’ directory.
   `
   user@host# edit shared acp configuration ldap service-data
   `
7. Specify whether SRC ACP detects changes in the backbone congestion point for a service while SRC ACP is operative.
   `
   [edit shared acp configuration ldap service-data]
   user@host# set reload-congestion-points
   `

[Contents] [Prev] [Next] [Index] [Report an Error]