[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Color Mark Actions (SRC CLI)

You can configure color-mark actions to apply a TOS mark value based on the packet’s color. A color-mark can be applied to a packet after it exits a rate-limit hierarchy.

The type of action that you can create depends on the type policy rule. See Policy Information Model.

Use the following configuration statements to configure color actions:

`

policies group name list name rule name color-mark name {
  green-mark green-mark;
  yellow-mark yellow-mark;
  red-mark red-mark;
  mask mask;
  description description;
}

`

To configure a color mark action:

1. From configuration mode, enter the color mark action configuration. For example, in this procedure, cma is the name of the color action.
   `
   [edit]
   user@host# edit policies group junose_filter list in rule pr color cma
   `
2. (Optional) Specify the green-mark value.
   `
   [edit policies group junose_filter list in rule pr filter cma]
   user@host# set green-mark green-mark
   `
3. (Optional) Specify the yellow-mark value.
   `
   [edit policies group junose_filter list in rule pr filter cma]
   user@host# set yellow-mark yellow-mark
   `
4. (Optional) Specify the red-mark value.
   `
   [edit policies group junose_filter list in rule pr filter cma]
   user@host# set red-mark red-mark
   `
5. Specify the mask value to use when marking packets.
   `
   [edit policies group junose_filter list in rule pr filter cma]
   user@host# set mask mask
   `
6. (Optional) Enter a description for the color mark action.
   `
   [edit policies group junose_filter list in rule pr filter cma]
   user@host# set description description
   `
7. (Optional) Verify the color action mark configuration.

       [edit policies group junose_filter list in rule pr filter cma]
       user@host# show
       description mark green packets;
       green-mark 100;
       mask 255;

#### Related Topics

- Before You Configure SRC Policies
- Configuring Hierarchical Rate-Limit Actions (SRC CLI)
- Configuring Rate-Limit Actions (SRC CLI)
- Configuring Color Actions (SRC CLI)
- Dynamic Bandwidth Allocation Among Traffic Flows in SRC Policy Lists for JUNOSe Routing Platforms

[Contents] [Prev] [Next] [Index] [Report an Error]