[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring General Properties for the SDX SNMP Agent

Use the following configuration statements to configure general properties for the SDX SNMP agent:

`

snmp agent {
  trap-history-limit trap-history-limit;
  component-polling-interval component-polling-interval;
  protocol-log-level protocol-log-level;
}

`

To configure properties for the SDX SNMP agent:

1. From configuration mode, access the configuration statement that configures the SDX SNMP agent.
   `
   [edit]
   user@host# edit snmp agent
   `
2. (Optional) Specify the maximum number of elements stored in the SNMP trap history table.
   `
   [edit snmp agent]
   user@host# set trap-history-limit trap-history-limit
   `
3. (Optional) Specify the interval at which an SRC component is polled.
   `
   [edit snmp agent]
   user@host# set component-polling-interval component-polling-interval
   `
4. (Optional) Specify the log level for SNMP requests and responses received from the master agent.
   `
   [edit snmp agent]
   user@host# set protocol-log-level protocol-log-level
   `

   To enable packet-level logging, set the protocol-log-level option to 9 or less.

5. (Optional) Verify your configuration.

       [edit snmp agent]
       user@host# show

   The output indicates the trap history limit, the component polling interval, the protocol log level, the initial properties, the logging destinations, and the Java heap size.

#### Related Topics

- Configuring the SDX SNMP Agent
- Configuring General Properties for the SDX SNMP Agent (C-Web Interface)
- Monitoring the SDX SNMP Agent

[Contents] [Prev] [Next] [Index] [Report an Error]