[Contents] [Prev] [Next] [Index] [Report an Error]

# Adding Operative JUNOS Routing Platforms

To add to the directory routers and JUNOS VRs that are currently operative and have an operating SNMP agent:

1. Click Manage>Request>Network>Discovery.
2. Enter information as described in the Help text in the main pane, and click Apply.

If you add a router using the discover network feature, the software adds the IP address of the first SNMP agent on the router to respond to the discover request.

#### Related Topics

- Overview of Adding JUNOS Routing Platforms and Virtual Routers
- Configuring the SAE to Manage JUNOS Routing Platforms (C-Web Interface)
- Configuring Secure Connections Between the SAE and JUNOS Routing Platforms
- Adding JUNOS Routers Individually
- Adding Virtual Routers Individually

[Contents] [Prev] [Next] [Index] [Report an Error]