[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring NIC to Store Log Messages in a File (C-Web Interface)

To configure component logging for NIC:

1. Click Configure, expand Shared, and then click NIC.

   The NIC pane appears.

2. In the side pane, expand a configuration scenario, such as Scenario:OnePopSharedlp.
3. In the side pane, expand a host, such as Demohost.

   The Hosts pane appears.

4. From the Create new list, select Logger.

   The name of the logger appears in the side pane and the Logger pane.

5. Expand the logger in the side pane, and then click File or Syslog.
6. Click Create, enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring a Component to Store Log Messages in a File (SRC CLI)
- Configuring ACP to Store Log Messages in a File (C-Web Interface)
- Configuring the SAE to Store Log Messages in a File (C-Web Interface)
- Configuring the SNMP to Store Log Messages in a File (C-Web Interface)
- Configuring JPS to Store Log Messages in a File (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]