[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Information About Subscribers Obtained from External Applications (C-Web Interface)

#### Purpose

View information about subscribers obtained from external applications with the C-Web interface.

#### Action

To view information about subscribers obtained from external applications:

1. Click ACP>Remote Update>Subscriber.

   The Remote Update/Subscriber pane appears.

2. In the Device Name box, enter the device name of the congestion point, or leave the box blank to display information about all devices.
3. In the NAS IP box, enter the NAS IP address of the device connected to the subscriber, or leave the box empty to display information about all subscribers.
4. In the NAS Port ID box, enter the NAS port ID connected to the subscriber, or leave the box empty to display information about all subscribers.
5. In the Phone box, enter the phone number of the subscriber, or leave the box blank to display information about all subscribers.
6. In the Slot box, enter the number of the slot for which you want to display external subscriber information.
7. Select an output style from the Style list.
8. In the Subscriber IP box, enter the subscriber IP address, or leave the box empty to display information about all subscribers.
9. Click OK.

   The Remote Update/Subscriber pane displays the congestion points.

#### Related Topics

- Viewing Information About Congestion Points from an External Application by DN (C-Web Interface)
- Viewing Information About Congestion Points from an External Application by Interface Name (C-Web Interface)
- Viewing Information About Edge Congestion Points by Subscriber Session (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]