> - Downloads
> - Configuration Tasks for Integrating Third-Party Network Devices
> - Related Topics
> - Configuration Tasks for Integrating Third-Party Network Devices (C-Web Interface)
> - Overview of Integrating Network Devices into the SRC Network
> - Logging In Subscribers and Creating Sessions

> # Configuration Tasks for Integrating Third-Party Network Devices

> To integrate third-party devices into your SRC network, complete the following tasks:

> - Write a script and add a script service that references the script.

>   See Setting Up Script Services .

> - Add objects for the devices.

>   See Adding Objects for Network Devices .

> - Configure an SAE community.

>   See Setting Up SAE Communities .

> - (Optional) Configure SAE properties for the Event Notification API if you are using the event notification method to log in subscribers.

>   See Configuring SAE Properties for the Event Notification API (SRC CLI).

> - Configure the session store.

>   See Storing Subscriber and Service Session Data.

> - If you are using the event notification method to log in subscribers, integrate the SAE with an IP address manager. There are two ways to do so:
>   - Use the event notification API to create an application that notifies the SAE when events occur between the DHCP server and the network device.

> See the event notification API documentation in the SAE CORBA remote API documentation on the Juniper Networks Web site at http://www.juniper.net/techpubs/software/management/src/api-index.html

> - Use Monitoring Agent, a sample application that was created with the event notification API and that monitors DHCP or RADIUS messages for DHCP or RADIUS servers.

> See the SRC PE Sample Applications Guide.

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.