[Contents] [Prev] [Next] [Index] [Report an Error]

# Verifying System Status

You can use show commands to check system status and monitor system activity.

To help you become familiar with show commands:

1. Type show ? to display the list of show commands that you can use to monitor the SRC software and C Series Controller.

       user@host> show ?
       Possible completions:
         acp                  Display information about ACP
         cli                  Configure properties for the CLI environment
         component            Display information about SRC components
         configuration        Information about the SRC configuration
         date                 System time and date
         disk                 Configuration for RAID disks
         interfaces           Show interface information
         iptables             Display information about the iptables LINUX tool
         jps                  Display information about the JPS
         nic                  Display information about the NIC
         ntp                  NTP configuration information
         redirect-server      Statistics for redirect server
         route                Show routing table information
         sae                  Display SAE information
         security             Display security information
         system               Display system information

2. Use the show component command to view a the status of installed components.

       user@host> show component
       Installed Components
       Name      Version                                            Status
       cli       Release: 7.0 Build: CLI.A.7.0.0.0171               running
       acp       Release: 7.0 Build: ACP.A.7.0.0.0174               disabled
       jdb       Release: 7.0 Build: DIRXA.A.7.0.0.0176             running
       editor    Release: 7.0 Build: EDITOR.A.7.0.0.0176            disabled
       redir     Release: 7.0 Build: REDIR.A.7.0.0.0176             disabled
       licSvr    Release: 7.0 Build: LICSVR.A.7.0.0.0179            stopped
       nic       Release: 7.0 Build: GATEWAY.A.7.0.0.0170           disabled
       sae       Release: 7.0 Build: SAE.A.7.0.0.0166               running
       www       Release: 7.0 Build: UMC.A.7.0.0.0169               disabled
       jps       Release: 7.0 Build: JPS.A.7.0.0.0172               disabled
       agent     Release: 7.0 Build: SYSMAN.A.7.0.0.0174            disabled
       webadm    Release: 7.0 Build: WEBADM.A.7.0.0.0173            disabled

3. Use the show system information command to view general system information.

       user@host> show system information
       System Identification
       Hostname         myCSeriesController
       Manufacturer     Juniper Networks
       Product Name     C-2000
       Version          1.0
       Serial Number    0207082006000001
       UUID             48384441-5254-0030-4859-0030485977EE
       Hostid           e30a2e07
       Software version SRC Release 2.0

       System Time
       Current time              2006-12-19 13:52:26 EST
       Uptime                    21:30
       Number of active users    3
       Load Averages (1m/5m/15m) 0.02/0.07/0.02

       Memory
       Total 15G
       Free  14G

       CPU Info
       Number of CPU 4
       CPU Model     Dual Core AMD Opteron(tm) Processor 265
       Clock Speed   1804.132 MHz
       Disk Information
         Mountpoint       Total Used  Use%
         /                2015M  955M  47%
         /altroot         2015M   35M   1%
         /altvar            29G   75M   0%
         /boot              98M   14M  14%
         /var               31G  829M   2%

       Temperature
       System +24 C
       CPU-1  +34 C
       CPU-2  +36 C

       Fan Speed
       Fan-1 9375 RPM
       Fan-2 9375 RPM

#### Related Topics

- Viewing C Series Controller Information
- Viewing Settings for the SRC CLI
- Viewing Information About the SRC CLI
- Overview of Configuration for the SRC CLI

[Contents] [Prev] [Next] [Index] [Report an Error]