[Contents] [Prev] [Next] [Index] [Report an Error]

# Creating an Application to Update Information for SRC ACP

You can develop your own application to update information about subscribers and congestion points for SRC ACP. The application can call one method to interact with SRC ACP. This method is called:

update (in RemoteUpdateType rut, in TagValueList attrs)

The method takes a property-value pair and passes the information to SRC ACP. For information about the properties and values you can pass to SRC ACP, see the file acpPlugin.idl in the folder SDK/idl in the `SDK+AppSupport+Demos+Samples.tar.gz` file on the Juniper Networks Web site at: https://www.juniper.net/support/csc/swdist-erx/src.html .

To create an application that updates SRC ACP remotely:

1. Compile the IDL file, and generate the code in the language in which you want to write the application.
2. Write the application, and include the generated code for the IDL file.
3. Use the CORBA object reference defined in the property ACP.syncRateAdaptor.ior to send data from the application to SRC ACP.

For information about the interfaces, properties, and methods available in the CORBA remote API for ACP, see the documentation in in the `SDK+AppSupport+Demos+Samples.tar.gz` file on the Juniper Networks Web site at: https://www.juniper.net/support/csc/swdist-erx/src.html . The files are in the SDK/doc/idl/acp/html/index.html directory.

#### Related Topics

- Overview of SRC ACP
- Interactions Between SRC ACP and Other Components
- Allocating Bandwidth to Applications Not Controlled by SRC ACP
- Use of Multiple SRC ACPs

[Contents] [Prev] [Next] [Index] [Report an Error]