[Contents] [Prev] [Next] [Index] [Report an Error]

# Adding Objects for CMTS Devices (SRC CLI)

To manage CMTS devices, the SAE creates and manages pseudointerfaces that it associates with a virtual router object. Each CMTS device in the SRC network must appear in the configuration as a router object, and it must be associated with a virtual router object called default. The router and virtual router are not actually configured on the CMTS device; the router and virtual router provide a way for the SAE to manage the CMTS device by using the SAE’s embedded policy server.

Use the following configuration statements to add a router object:

`

shared network device name {
  description description ;
  management-address management-address ;
  device-type (junose | junos | pcmm | proxy);
  qos-profile [ qos-profile ...];
}

`

To add a router:

1. From configuration mode, access the configuration statements that configure network devices. You must specify the name of a device with lowercase characters. In this sample procedure, pcmm_dtr is the name of the object.
   `
   user@host# edit shared network device pcmm_dtr
   `
2. (Optional) Add a description for the CMTS device.
   `
   [edit shared network device pcmm_dtr]
   user@host# set description description
   `
3. Add the IP address of the CMTS device.
   `
   [edit shared network device pcmm_dtr]
   user@host# set management-address management-address
   `
4. (Optional) Specify the type of device that you are adding.
   `
   [edit shared network device pcmm_dtr]
   user@host# set device-type pcmm
   `
5. (Optional) Verify your configuration.

       [edit shared network device pcmm_dtr]
       user@host# show
       description "CMTS device";
       management-address 192.168.3.5;
       device-type pcmm;
       interface-classifier {
         rule rule-0 {
           script #;
         }
       }

#### Related Topics

- Connections to Managed Devices
- Configuring CMTS-Specific RKS Plug-Ins (SRC CLI)
- Creating Virtual Routers for the CMTS Device (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]