> - Downloads
> - Viewing Statistics for All JUNOSe Device Drivers (SRC CLI)
> - Related Topics
> - Troubleshooting Problems with Managing JUNOSe Routers
> - Viewing Statistics for Specific JUNOSe Device Drivers (SRC CLI)
> - Viewing the State of JUNOSe Device Drivers (C-Web Interface)
> - Viewing Statistics for All JUNOSe Device Drivers (C-Web Interface)

> # Viewing Statistics for All JUNOSe Device Drivers (SRC CLI)

> #### Purpose

> Display SNMP statistics for all JUNOSe device drivers.

> #### Action

> Use the following operational mode command:

> `
> show sae statistics device common junose-cops
> `

> For example:

> `user@host> show sae statistics device common junose-cops`

>     SNMP Statistics
>     Driver type                    JUNOSE COPS
>     Number of close requests       0
>     Number of connections accepted 2
>     Number of current connections  1
>     Number of open requests        2
>     Server address                 0:0:0:0:0:0:0:0
>     Server port                    3288
>     Time since last redirect       186703

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.