[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the JUNOS Routing Platform to Apply Changes It Receives from the SAE

To configure the JUNOS routing platform to receive configuration statements from the SAE and apply those statements to the configuration:

1. Create a configuration group called sdx that contains the configuration statements that the SAE sends to the JUNOS routing platform. To do so, include the groups statement at the [edit] level, and specify the name sdx.
   `
   [edit]
   groups {
     sdx;
   }
   `
2. Configure the JUNOS routing platform to apply these statements to the configuration. To do so, include the apply-groups statement at the [edit] level.
   `
   [edit]
   set apply-groups sdx;
   `

#### Related Topics

- Configuring JUNOS Routing Platforms to Interact with the SAE
- Disabling Interactions Between the SAE and JUNOS Routing Platforms
- Monitoring Interactions Between the SAE and JUNOS Routing Platforms
- Checking Changes to the JUNOS Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]