> - Downloads
> - Viewing the State of JUNOS Device Drivers (SRC CLI)
> - Related Topics
> - Viewing the State of JUNOS Device Drivers (C-Web Interface)
> - Troubleshooting Problems with the SRC Software Process
> - Viewing Statistics for Specific JUNOS Device Drivers (SRC CLI)
> - Viewing Statistics for All JUNOS Device Drivers (SRC CLI)

> # Viewing the State of JUNOS Device Drivers (SRC CLI)

> #### Purpose

> Display the state of JUNOS drivers.

> #### Action

> Use the following operational mode command:

> `
> show sae drivers <device-name device-name > < (brief) > <maximum-results maximum-results >
> `

> For example:

> `user@host> show sae drivers device-name default@jrouter`

>     JUNOS Driver
>     Device name                           default@jrouter
>     Device type                           junos
>     Device IP                             /10.10.6.113:1879
>     Local IP                              10.10.6.113
>     TransportRouter
>     Device version                        8.2R1.7
>     Start time                            Thu Mar 08 21:00:50 UTC 2007
>     Number of notifications               0
>     Number of processed added             0
>     Number of processed changed           0
>     Number of processed deleted           0
>     Number of provisioning attempt        0
>     Number of provisioning attempt failed 0
>     Device type                           JunosRouterDriver
>     Job queue size                        0
>     Number of SAP                         3
>     Number of PAP                         0
>     Start time                            Thu Mar 08 21:00:55 UTC 2007
>     End time                              Thu Mar 08 21:00:55 UTC 2007
>       Transaction Manager
>       Transaction queue size 0
>       Router name            default@troll

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.