[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Protocol Conditions (C-Web Interface)

The procedure in this sections shows how to configure general protocol conditions.

- If your condition includes port numbers, use the procedure in Configuring Protocol Conditions with Ports (C-Web Interface).
- If your condition consists of a protocol that is assigned with a parameter value, use the procedure in Configuring Protocol Conditions with Parameters (C-Web Interface).

To configure general protocol conditions in a classify-traffic condition:

1. In the side pane, expand a traffic condition, and select Protocol Condition.
2. Click Create, enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring Protocol Conditions (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]