[Contents] [Prev] [Next] [Index] [Report an Error]

## NIC Performance Traps

Table 10 lists the performance traps for NIC.

Table 10: Performance Traps–NIC

|  |  | Alarm Threshold Levels (default values) |
--- | --- | --- | --- | ---
Trap Event | Trap ID | Text Displayed | Critical | Major | Minor | Interval(sec) | R/AV
nicHostReslvErrors | 230 | $S:NIC Host: During the last $Ps, the number of resolution errors that occurred is $D. This $L is the threshold of $T errors.:$A | 10 | 5 | 1 | 60 | R
nicHostAvgReslvTime | 231 | $S:NIC Host: During the last $Ps, the average time this NIC Host spent on resolutions is $Dms. This $L the threshold of $Tms.:$A | 1000 | 500 | 250 | 60 | R

#### Related Topics

- Performance Traps
- Trap Numbers in Performance Traps
- Configuring Performance Traps

[Contents] [Prev] [Next] [Index] [Report an Error]