[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Access Control for SNMPv3 Users (C-Web Interface)

To configure access control for SNMPv3 users:

1. Click Configure, and expand SNMP>V3>USM>Local Engine.
2. From the Create new list, select User.
3. Enter a name for the new User in the dialog box, and click OK.
4. From the side pane, expand the name of the user, and (optional) specify the authentication type and (optional) the encryption.

   | Note: Before you configure encryption, you must configure the authentication type.

#### Related Topics

- Configuring an SNMPv3 Security Name for SNMP Monitoring (SRC CLI)
- Configuring Access Control for SNMPv3 Users (C-Web Interface)
- Configuring Authentication
- Configuring Access Control for Communities

[Contents] [Prev] [Next] [Index] [Report an Error]