[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Information About Edge Congestion Points by DN (C-Web Interface)

#### Purpose

View information about edge congestion points by DN.

#### Action

To view information about edge congestion points:

1. Click ACP>Edge>Congestion Point>DN.

   The Edge/Congestion Point/DN pane appears.

2. In the Congestion Point DN box, enter a congestion point DN, or leave the box blank to view information for all DNs.
3. In the Slot box, enter the number of the slot for which you want to display congestion point information.
4. Select an output style from the Style list.
5. In the Virtual Router Name box, enter a virtual router name to display information about a specific virtual router, or leave the box empty to display information about all virtual routers.
6. Click OK.

   The Edge/Congestion Point/DN pane displays a list of congestion points.

#### Related Topics

- Configuring SRC ACP to Manage the Edge Network (C-Web Interface)
- Viewing Information About Edge Congestion Points by DN (C-Web Interface)
- Viewing Information About Edge Congestion Points by Subscriber Session (C-Web Interface)
- Viewing Information About Subscriber Sessions in the Edge Network (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]