[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring NIC Replication (C-Web Interface)

You configure NIC replication to keep the NIC configuration highly available.

Before you configure NIC replication:

- Make sure that you understand how NIC groups are used.

  See Locating Subscriber Management Information.

- Identify which NIC hosts are to provide redundancy for each other.
- Specify a name for a group for each of these hosts.

To configure NIC replication:

1. Click Configure>Slot, then a specified slot (for example, slot0), and then NIC.

   The NIC pane appears.

2. Specify a group for NIC replication in the Runtime Group box, as described in the Help text; for example, group1.
3. Click Apply.
4. In the left pane, click Commit.

#### Related Topics

- Configuring the NIC (C-Web Interface)
- Reviewing and Changing Operating Properties for NIC (C-Web Interface)
- High Availability for NIC

[Contents] [Prev] [Next] [Index] [Report an Error]