[Contents] [Prev] [Next] [Index] [Report an Error]

# Defining an Alarm to Monitor the Status of an Object (SRC CLI)

You can configure a monitor to identify when a MIB object appears, disappears, or changes value. If the test criteria are met, the test is considered to be successful.

| Note: Configure only one monitor test at a time.

Before you define an alarm type, configure the associated SNMP alarm.

See Configuring an SNMP Alarm on a C Series Controller (SRC CLI).

To configure an alarm to monitor the status of an object:

- Specify the type of alarm: present, absent, or changed. For example for an alarm named existence-alarm:
  `
  [edit snmp monitor alarm existence-alarm existence-test]
  user@host# set type present
  `

#### Related Topics

- Defining an Alarm for an SNMP Monitor That Compares Object Values (SRC CLI)
- Defining an Alarm for an SNMP Monitor That Compares Values Against Thresholds (SRC CLI)
- Configuring an SNMP Alarm on a C Series Controller (SRC CLI)
- Configuration Statements for Customized SRC SNMP Monitors
- SNMP Monitoring on C Series Controllers

[Contents] [Prev] [Next] [Index] [Report an Error]