> - Downloads
> - Configuration Statements for SRC CLI Directory Access
> - Related Topics
> - Changing Access to the Directory that Stores SRC Configuration Data
> - Overview of Configuration for the SRC CLI

> ## Configuration Statements for SRC CLI Directory Access

> Use the following configuration statements to change the connection to the directory that stores SRC configuration information. You enter the system ldap client statement at the [edit] hierarchy level:

> `
> system ldap client {
>   base-dn base-dn ;
>   url url ;
>   backup-urls backup-urls ;
>   authentication-dn authentication-dn ;
>   credentials credentials ;
>   connect-timeout connect-timeout ;
>   time-limit time-limit ;
>   eventing;
>   polling-interval polling-interval ;
>   connection-manager-id connection-manager-id ;
>   dispatcher-pool-size dispatcher-pool-size ;
>   event-base-dn event-base-dn ;
>   signature-dn signature-dn ;
>   blacklist;
> }
> `

> | Note: Do not change the value for the enable-eventing, polling-interval, connection-manager-id, dispatcher-pool-size, or event-base-dn statements unless instructed to do so by Juniper Networks. The eventing statement is enabled by default.

> #### Published: 2009-09-25

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.