[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Congestion Point Classification (C-Web Interface)

Congestion point classification allows you to automate and scale the configuration of congestion points. SRC ACP uses classification scripts to determine which congestion point to load for a subscriber. SRC ACP can select the congestion point from congestion point profiles or subscriber profiles.

To configure congestion point classification scripts:

- Configuring Targets and Criteria for Classification Scripts
- Configuring Classification Script Contents for Classification Scripts

## Configuring Targets and Criteria for Classification Scripts

To define a target and criteria for the congestion point classification script:

1. Click Configure>Shared>ACP>Configuration >Scripts and Classification.

   The Scripts and Classification pane appears.

2. Click Create, enter information as described in the Help text in the main pane, and click Apply.

## Configuring Classification Script Contents for Classification Scripts

To use the contents of a classification script to point to another object for the congestion point classification script:

1. Click Configure>Shared>ACP, expand the desired group, and click Congestion Point Classifier.

   The Congestion Point Classifier pane appears.

2. In the Create new list, select Rule.
3. Type a name for the new rule, and click OK.
4. In the side pane, expand the new rule, enter information for the script as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Classifying Congestion Points
- Configuring Congestion Point Classification (C-Web Interface)
- Overview of Congestion Point Classification

[Contents] [Prev] [Next] [Index] [Report an Error]