[Contents] [Prev] [Next] [Index] [Report an Error]

# Accessing the Router CLI

You can access the CLIs of Juniper Networks routers through a Telnet or secure shell connection.

- To open a Telnet session to a router, use the telnet operational mode command. For example:
  `
  user@host> telnet 10.10.10.3
  `
- To open a secure shell connection, use the ssh operational command. For example:
  `
  user@host> ssh host 10.10.10.3
  `

#### Related Topics

- Specifying Router Initialization Scripts on the SAE with the CLI
- Starting the SRC Client on a JUNOSe Router
- Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices

[Contents] [Prev] [Next] [Index] [Report an Error]