> - Downloads
> - Setting the Timeout and Number of Events for SAE Directory Eventing (C-Web Interface)
> - Related Topics
> - For information about setting up SAE groups, see Configuring an SAE Group.

> # Setting the Timeout and Number of Events for SAE Directory Eventing (C-Web Interface)

> To configure the directory eventing timeout and the number of simultaneous events that the SAE can receive from the directory:

> 1. Click Configure, expand Shared>SAE>LDAP, and then click Directory Eventing.

>    The Directory Eventing pane appears.

> 2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.