[Contents] [Prev] [Next] [Index] [Report an Error]

## Configuration Statements for Customized SRC SNMP Monitors

Use the following configuration statements to configure the SNMP custom monitoring at the [edit] hierarchy level.

`

snmp monitor {
  security-name security-name;
}
  snmp monitor alarm name{
    interval interval;
    sample-type (absolute-value | delta-value);
    ignore-startup-alarm;
    event event;
    variable variable;
    strict-oid;
  }
  snmp monitor alarm name boolean-test {
    comparison (equal | unequal | less | less-or- equal | greater | greater-or-equal);
    value value;
  }
  snmp monitor alarm name existence-test {
    type (present | absent | changed);
  }
  snmp monitor alarm name threshold-test {
    rising-threshold rising-threshold;
    falling-threshold falling-threshold;
  }
  snmp monitor alarm name delta-discontinuity-check {
    variable variable;
  }
  snmp monitor event namenotification {
    oid oid;
    strict-object [strict-object...];
    wildcarded-object [wildcarded-object...];
  }
  snmp monitor event name snmp-set {
    variable variable;
    value value;
    strict-oid;
  }

`

#### Related Topics

- Configuring an SNMP Alarm on a C Series Controller (SRC CLI)
- Example: SNMP Monitoring of Multiple MIB Objects
- Configuring an SNMPv3 Security Name for SNMP Monitoring (SRC CLI)
- SNMP Monitoring on C Series Controllers
- For detailed information about each configuration statement, see the SRC PE CLI Command Reference

[Contents] [Prev] [Next] [Index] [Report an Error]