[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Edge Congestion Point Information by DN

#### Purpose

View edge congestion point information by DN.

#### Action

To display information about edge congestion points by DN:

`user@host> show acp edge congestion-point dn`
`

`

To display information about specific congestion points by DN:

`user@host> show acp edge congestion-point dn congestion-point-dn congestion-point-dn`
`

`

Enter a partial congestion point DN to list all matching congestion points.

To display information about specific congestion points that were generated dynamically by instance ID:

`user@host> show acp edge congestion-point dn instance-id instance-id`
`user@host> show acp edge congestion-point dn congestion-point-dn congestion-point-dn instance-id instance-id`
`

`

When a congestion point is dynamically generated with a congestion point profile, the generated instance ID is appended to the congestion point DN. Enter a partial instance ID to list all matching congestion points.

To display information about the congestion points from a specific virtual router:

`user@host> show acp edge congestion-point dn virtual-router-name virtual-router-name`
`

`

Enter a virtual router name to list congestion points from a particular virtual router.

To display congestion point DNs:

`user@host> show acp edge congestion-point dn brief`
`

`

By default, information about the congestion point attributes and congestion point bandwidth usage is displayed.

To restrict the number of displayed results:

`user@host> show acp edge congestion-point dn maximum-results maximum-results`
`

`

#### Related Topics

- Configuring SRC ACP to Manage the Edge Network
- Viewing Information About Edge Congestion Points by DN (C-Web Interface)
- Viewing Edge Congestion Point Information by Subscriber Session

[Contents] [Prev] [Next] [Index] [Report an Error]