[Contents] [Prev] [Next] [Index] [Report an Error]

# Adding Virtual Routers Individually

To add a virtual router to an existing router:

1. Click Configure, expand Shared>Network, and then click a JUNOS router.

   The Device pane appears.

2. From the Create new list, select Virtual Router.
3. Type a name for the new device in the dialog box, and click OK.

   The Virtual Router pane appears.

4. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- For information about service scopes, see Configuring Service Scopes (SRC CLI)
- Overview of Adding JUNOS Routing Platforms and Virtual Routers
- Adding the Server Certificate on the Routing Platform
- Adding the Client Certificate on the Router
- Adding Operative JUNOS Routing Platforms
- Adding JUNOS Routers Individually

[Contents] [Prev] [Next] [Index] [Report an Error]