[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Loss Priority Actions (C-Web Interface)

You can configure loss priority actions for JUNOS filter policy rules. The loss priority action causes the router to assign a packet loss priority to packets that match the associated classify-traffic condition.

To configure a loss priority action:

1. In the side pane, select a JUNOS filter rule.
2. From the Create new list, select Loss Priority. Type a name for the action, and click OK.
3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Delivering QoS Services in a Cable Environment
- Configuring Loss Priority Actions (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]