[Contents] [Prev] [Next] [Index] [Report an Error]

## Parameter Values Used by Services for Exceptions to Stateless Firewalls

Table 13 lists the parameters for which Enterprise Manager Portal provides values. The parameter names start with “ fw” (service’s LDAP attribute parameterSubstitution). The services listed in Before You Configure Services for Enterprise Manager Portal use these parameters.

Table 13: Parameters for Stateless Firewall Services for Enterprise Manager Portal

To Specify this Value | Use This Parameter
--- | ---
Protocol | fwProtocol
Source network | fwSrcIp
Source port | fwSrcPort
Destination network | fwDestIp
Destination port | fwDestPort
TOS byte | fwTosByte
TOS byte mask | fwTosByteMask
TCP flags | fwTcpFlags
TCP flags mask | fwTcpFlagsMask
IP flags | fwIpFlags
IP flags mask | fwIpFlagsMask
Fragmentation offset | fwIpFragOffset
ICMP type | fwIcmpType
ICMP code | fwIcmpCode
Packet length | fwPacketLength

[Contents] [Prev] [Next] [Index] [Report an Error]