[Contents] [Prev] [Next] [Index] [Report an Error]

# Disabling an SRC Component

On a C Series Controller, you can disable a module or component that is running from the CLI.

To disable a component:

1. Verify which components are running by entering the show component command in operation mode:

       user@host> show component
       Installed Components
       Name      Version                                            Status
       cli       Release: 7.0 Build: CLI.A.7.0.0.0171               running
       acp       Release: 7.0 Build: ACP.A.7.0.0.0174               disabled
       jdb       Release: 7.0 Build: DIRXA.A.7.0.0.0176             running
       editor    Release: 7.0 Build: EDITOR.A.7.0.0.0176            disabled
       redir     Release: 7.0 Build: REDIR.A.7.0.0.0176             disabled
       licSvr    Release: 7.0 Build: LICSVR.A.7.0.0.0179            stopped
       nic       Release: 7.0 Build: GATEWAY.A.7.0.0.0170           disabled
       sae       Release: 7.0 Build: SAE.A.7.0.0.0166               running
       www       Release: 7.0 Build: UMC.A.7.0.0.0169               disabled
       jps       Release: 7.0 Build: JPS.A.7.0.0.0172               disabled
       agent     Release: 7.0 Build: SYSMAN.A.7.0.0.0174            disabled
       webadm    Release: 7.0 Build: WEBADM.A.7.0.0.0173            disabled

2. Disable a component by using the disable component command in operational mode. For example:
   `
   user@host> disable sae
   `

#### Related Topics

- Enabling SRC Components
- Restarting an SRC Module or Component
- Configuring SRC Components

[Contents] [Prev] [Next] [Index] [Report an Error]