> - Downloads
> - Defining Access Privileges for an SNMP Group (C-Web Interface)
> - Related Topics
> - Defining Access Privileges for an SNMP Group
> - Assigning Security Names to Groups (C-Web Interface)
> - Configuring Access Control for the VACM (C-Web Interface)

> # Defining Access Privileges for an SNMP Group (C-Web Interface)

> To configure MIB views with a group for the VACM:

> 1. Click Configure, and expand SNMP>V3>VACM>Access.
> 2. From the Create new list, select Group.
> 3. Enter a name for the new Group in the dialog box, and click OK.

>    The group name is the name for a collection of SNMP security names that belong to the same SNMP access policy.

> 4. From the side pane, expand the name of the group, click on Default Context Prefix,
> 5. From the Create New box, select the Security Model for access privileges.
> 6. From the Create New box, select the Security Level for access privileges.

>    The Security pane appears.

> 7. Enter information as described in the Help text in the main pane, and then click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.